Founday Shop Procedure:

Pattern was put in drag. Parting sand was applied. Wooden pattern bounded by the silicon clay.

Hammering done by round rammer and peen rammer to remove excessive sand